DICOM PS3.3 2018d - Information Object Definitions

10.25.2 Constraint Violation Significance (Current)
Prev | 10.25 Attribute Value Constraint Macro | Next

### 10.25.2 Constraint Violation Significance

The violation of some constraints may be more significant than others. Constraint Violation Significance (0082,0036) differentiates three levels of signficance.

Specific behaviors associated with each level may be defined by the SOP Class or may be left to implementations. For example, violation of a constraint with a significance of FAILURE might require operator intervention, special auditing or rejection of the target instance being evaluated; violation of a constraint with a significance of WARNING might require the operator be notified or a warning message be logged; violation of a constraint with a significance of INFORMATIVE might require an informational message be logged, or nothing at all if the constraint represents a preference not a signficant concern.

### Note

Violation of a constraint does not imply that the Selector Attribute value is non-conformant to the Standard or is not clinically appropriate.

Prev | Up | Next
10.25 Attribute Value Constraint Macro | Home | 10.26 Attribute Value Macro

DICOM PS3.3 2018d - Information Object Definitions