DICOM PS3.3 2018d - Information Object Definitions

C.8.13.5.11 MR Spatial Saturation Macro (Current)
Prev | C.8.13.5 Enhanced MR Image Functional Group Macros | Next

##### C.8.13.5.11 MR Spatial Saturation Macro

Table C.8-98 specifies the Attributes of the MR Spatial Saturation Functional Group Macro.

Table C.8-98. MR Spatial Saturation Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
MR Spatial Saturation Sequence | (0018,9107) | 2 | A Sequence that provides the position of spatial saturation bands deposited as part of the pulse sequence. Zero or more Items shall be included in this Sequence.
>Slab Thickness | (0018,9104) | 1 | Thickness of slab in mm.
>Slab Orientation | (0018,9105) | 1 | The direction cosines of a normal vector perpendicular to the saturation plane with respect to the patient. See Section C.7.6.2.1.1 for further explanation.
>Mid Slab Position | (0018,9106) | 1 | The x, y, and z coordinates of the midpoint of the slab plane in mm with respect to the patient. See Section C.7.6.2.1.1 for further explanation.

Prev | Up | Next
C.8.13.5.10 MR Averages Macro | Home | C.8.13.5.12 MR Metabolite Map Macro

DICOM PS3.3 2018d - Information Object Definitions