DICOM PS3.16 2018d - Content Mapping Resource

TID 4126 Colon CAD Composite Feature Body (Current)
Prev | Colon CAD SR IOD Templates | Next

### TID 4126 Colon CAD Composite Feature Body

The details of a composite feature are expressed in this Template. It is applied to Colon CAD Composite Feature (TID 4125 “Colon CAD Composite Feature”).

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4126. Colon CAD Composite Feature Body

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (111016, DCM, "Composite type") | 1 | M |  | DCID 6035 “Composite Feature Relations”
2 |  |  | CODE | EV (111057, DCM, "Scope of Feature") | 1 | M |  | DCID 6036 “Scope of Feature”
3 |  |  | NUM | EV (111011, DCM, "Certainty of feature") | 1 | U |  | UNITS = EV (%, UCUM, "Percent") Value = 0 - 100
4 |  |  | INCLUDE | DTID 4129 “Colon CAD Geometry” | 1 | U |  |
5 |  |  | INCLUDE | DTID 4128 “Colon CAD Descriptors” | 1 | U |  |
6 |  |  | NUM | DCID 6207 “Colon Quantitative Temporal Difference Type” | 1-n | UC | May be present IFF the value of row 1 is (111153, DCM, "Target content items are related temporally") |
7 | > | R-INFERRED FROM | NUM |  | 2 | U |  | The referenced numeric values shall have the same Concept Name. Their UNITS shall be the same as row 6
8 |  |  | CODE | EV (111049, DCM, "Qualitative Difference") | 1-n | UC | May be present only if the value of row 1 is (111153, DCM, "Target content items are related temporally") | DCID 6134 “Chest Qualitative Temporal Difference Type”
9 | > | HAS PROPERTIES | TEXT | EV (111021, DCM, "Description of Change") | 1 | U |  |
10 | > | R-INFERRED FROM | CODE |  | 2 | M |  | The referenced Content Items shall have the same Concept Name and their code values shall be from the same context group.

Content Item Descriptions

Certainty of Feature | The CAD device's certainty that the feature analyzed and classified by the CODE, as specified in the Composite Feature parent Template is, in fact, that type of feature.
Row 6 | Values ≤ 0 are allowed. The two referenced numeric values are Target Content Items of the first generation Composite Feature or Single Image Finding children of this composite feature. Given the equation, A - B, the value representing A shall be referenced first.
Qualitative Difference | The two referenced code values are Target Content Items of the first generation Composite Feature or Single Image Finding children of this composite feature.

Prev | Up | Next
TID 4125 Colon CAD Composite Feature | Home | TID 4127 Colon CAD Single Image Finding

DICOM PS3.16 2018d - Content Mapping Resource