DICOM PS3.2 2018d - Conformance

E.8.5.2 Standard Extended Basic Film Box SOP Class (Current)
Prev | E.8.5 Standard Extended / Specialized / Private SOP Classes | Next

#### E.8.5.2 Standard Extended Basic Film Box SOP Class

SOP Class : Basic Film Box SOP

Attribute : Film Size (2010,2010)

Extensions : CURRENT

This extension allows images to be printed on whatever film size is currently loaded in the printer.

Note that if Film Size is specified, and a size other than that requested is installed, the EXAMPLE-PRINT-SERVER-MANAGEMENT will return success (0x0), and will either queue the print job until the correct sized film is installed or print on the media currently installed, based on the EXAMPLE-PRINT-SERVER-MANAGEMENT configuration. Specifying the Film Size to CURRENT will ensure that the print job will always be printed.

If Film Size is not specified, then the default CURRENT will be used, allowing images to always be printed.

Prev | Up | Next
E.8.5 Standard Extended / Specialized / Private SOP Classes | Home | E.8.5.3 Standard Extended Basic Grayscale Image Box SOP Class

DICOM PS3.2 2018d - Conformance