DICOM PS3.17 2018d - Explanatory Information

S.2 Managed Association Requester, Legacy Association Acceptor (Current)
Prev | S Legacy Transition For Configuration Management (Informative) | Next

## S.2 Managed Association Requester, Legacy Association Acceptor

### S.2.1 DHCP Server

The DHCP server may need to be configured with a pre-assigned IP address for the Association Requester if the legacy Association Acceptor restricts access by IP addresses. Otherwise no special actions are needed.

Prev | Up | Next
S Legacy Transition For Configuration Management (Informative) | Home | S.2.2 DNS Server

DICOM PS3.17 2018d - Explanatory Information