DICOM PS3.4 2018d - Service Class Specifications

B.2 Behavior (Current)
Prev | B Storage Service Class (Normative) | Next

## B.2 Behavior

This Section discusses the SCU and SCP behavior for SOP Classes of the Storage Service Class. The C-STORE DIMSE-C Service shall be the mechanism used to transfer SOP Instances between peer DICOM AEs as described in PS3.7.

### B.2.1 Behavior of an SCU

The SCU invokes a C-STORE DIMSE Service with a SOP Instance that meets the requirements of the corresponding IOD. The SCU shall recognize the status of the C-STORE service and take appropriate action upon the success or failure of the service.

### Note

The appropriate action is implementation dependent. It is required that the SCU distinguish between successful and failed C-STORE responses. Appropriate action may differ according to application, but are described in the Conformance Statement of the SCU.

Prev | Up | Next
B Storage Service Class (Normative) | Home | B.2.2 Behavior of an SCP

DICOM PS3.4 2018d - Service Class Specifications