DICOM PS3.3 2018d - Information Object Definitions

A.33.3.3 Pseudo-color Softcopy Presentation State IOD Module Table (Current)
Prev | A.33.3 Pseudo-color Softcopy Presentation State IOD | Next

#### A.33.3.3 Pseudo-color Softcopy Presentation State IOD Module Table

Table A.33.3-1 specifies the Modules of the Pseudo-color Softcopy Presentation State IOD.

Table A.33.3-1. Pseudo-Color Softcopy Presentation State IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Presentation Series | C.11.9 | M
Equipment | General Equipment | C.7.5.1 | M
Presentation State | Presentation State Identification | C.11.10 | M
Presentation State Relationship | C.11.11 | M
Presentation State Shutter | C.11.12 | M
Presentation State Mask | C.11.13 | M
Mask | C.7.6.10 | C - Required if the referenced image(s) are multi-frame and are to be subtracted
Display Shutter | C.7.6.11 | C - Required if a Display Shutter is to be applied to referenced image(s) and the Bitmap Display Shutter Module is not present
Bitmap Display Shutter | C.7.6.15 | C - Required if a Display Shutter is to be applied to referenced image(s) and the Display Shutter Module is not present
Overlay Plane | C.9.2 | C - Required if Overlay is to be applied to referenced image(s) or the Bitmap Display Shutter Module is present
Overlay Activation | C.11.7 | C - Required if referenced image contains overlay data that is to be displayed or Presentation State Instance contains Overlay data other than Bitmap Shutter
Displayed Area | C.10.4 | M
Graphic Annotation | C.10.5 | C - Required if Graphic Annotations are to be applied to referenced image(s)
Spatial Transformation | C.10.6 | C - Required if rotation or flipping are to be applied to referenced image(s)
Graphic Layer | C.10.7 | C - Required if Graphic Annotations or Overlays or Curves are to be applied to referenced image(s)
Graphic Group | C.10.11 | U
Modality LUT | C.11.1 | C - Required if a Modality LUT is to be applied to referenced image(s)
Softcopy VOI LUT | C.11.8 | C - Required if a VOI LUT is to be applied to referenced image(s)
Palette Color Lookup Table | C.7.9 | M
ICC Profile | C.11.15 | M
SOP Common | C.12.1 | M

In the Pseudo-Color Softcopy Presentation State IOD, the Presentation Series Module specializes some Attributes of the General Series Module, the Presentation State Mask Module specializes some Attributes of the Mask Module, and the Presentation State Shutter Module specializes some Attributes of the Bitmap Display Shutter Module and Display Shutter Module.

The Softcopy Presentation LUT Module shall not be present in this IOD.

Prev | Up | Next
A.33.3.2 Pseudo-color Softcopy Presentation State IOD Entity-Relationship Model | Home | A.33.4 Blending Softcopy Presentation State IOD

DICOM PS3.3 2018d - Information Object Definitions