DICOM PS3.3 2018d - Information Object Definitions

A.51.4 Segmentation IOD Content Constraints (Current)
Prev | A.51 Segmentation IOD | Next

### A.51.4 Segmentation IOD Content Constraints

The VOI LUT Module shall not be present.

The Modality LUT Module shall not be present.

The Overlay Plane Module shall not be present.

Pixel Padding Value (0028,0120) shall not be present.

The Defined CID for Purpose of Reference Code Sequence (0040,A170) within Source Instance Sequence (0042,0013) in the General Reference Module shall be CID 7019 “Segmentation Non-Image Source Purposes of Reference”.

Prev | Up | Next
A.51.3 Segmentation IOD Module Table | Home | A.51.5 Segmentation Functional Groups

DICOM PS3.3 2018d - Information Object Definitions