DICOM PS3.16 2018d - Content Mapping Resource

TID 4015 CAD Detections Performed (Current)
Prev | Mammography CAD SR IOD Templates | Next

### TID 4015 CAD Detections Performed

This Template gathers two lists of detection algorithms attempted, grouped by success/failure status. Algorithms not attempted are not mentioned in this sub-tree of the Document Root (e.g., TID 4000 “Mammography CAD Document Root”). This information forms the basis for understanding why a CAD report may produce no (or fewer than anticipated) detection results.

The sub-tree formed by this Template is illustrated in Figure E.1-2 “Summary of Detections and Analyses Levels of Mammography CAD SR Content Tree” in PS3.17 .

Table TID 4015. Parameters

Parameter Name | Parameter Usage
--- | ---
$DetectionCode | Coded term or Context Group for Detection Performed

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4015. CAD Detections Performed

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (111063, DCM, "Successful Detections") | 1 | MC | Shall be present only if value of parent is (111222, DCM, "Succeeded") or (111223, DCM, "Partially Succeeded") |
2 | > | CONTAINS | INCLUDE | DTID 4017 “CAD Detection Performed” | 1-n | M |  | $DetectionCode = $DetectionCode
3 |  |  | CONTAINER | EV (111025, DCM, "Failed Detections") | 1 | MC | Shall be present only if value of parent is (111224, DCM, "Failed") or (111223, DCM, "Partially Succeeded") |
4 | > | CONTAINS | INCLUDE | DTID 4017 “CAD Detection Performed” | 1-n | M |  | $DetectionCode = $DetectionCode

Prev | Up | Next
TID 4014 CAD Image Quality | Home | TID 4016 CAD Analyses Performed

DICOM PS3.16 2018d - Content Mapping Resource