DICOM PS3.3 2018d - Information Object Definitions

A.55.3 Breast Tomosynthesis Image IOD Module Table (Current)
Prev | A.55 Breast Tomosynthesis Image IOD | Next

### A.55.3 Breast Tomosynthesis Image IOD Module Table

Table A.55-1 specifies the Modules of the Breast Tomosynthesis Image IOD.

Table A.55-1. Breast Tomosynthesis Image IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Enhanced Mammography Series | C.8.11.10 | M
Frame of Reference | Frame of Reference | C.7.4.1 | M
Synchronization | C.7.4.2 | C - Required if time synchronization was applied.
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Image | Image Pixel | C.7.6.3 | M
Enhanced Contrast/Bolus | C.7.6.4b | C - Required if contrast media was applied.
Device | C.7.6.12 | U
Intervention | C.7.6.13 | U
Acquisition Context | C.7.6.14 | M
Multi-frame Functional Groups | C.7.6.16 | M
Multi-frame Dimension | C.7.6.17 | U
Image - Equipment Coordinate Relationship | C.7.6.21 | U
Specimen | C.7.6.22 | U
X-Ray 3D Image | C.8.21.1 | M
Breast Tomosynthesis Contributing Sources | C.8.21.2.3 | U
Breast Tomosynthesis Acquisition | C.8.21.3.4 | U
X-Ray 3D Reconstruction | C.8.21.4 | U
Breast View | C.8.21.6 | M
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U
Frame Extraction | C.12.3 | C - Required if the SOP Instance was created in response to a Frame-Level retrieve request

#### A.55.3.1 Breast Tomosynthesis Image IOD Content Constraints

##### A.55.3.1.1 Restrictions for Standard Extended SOP Classes

The Overlay Plane Module, Modality LUT Module, VOI LUT Module and Softcopy Presentation LUT Module shall not be used in a Standard Extended SOP Class of the Breast Tomosynthesis Image.

### Note

The VOI LUT function is provided by a Frame VOI LUT Functional Group.

##### A.55.3.1.2 Image - Equipment Coordinate Relationship Module

For Breast Tomosynthesis Image SOP Instances created from SOP Instances of the Breast Projection X-Ray Image SOP Classes (1.2.840.10008.5.1.4.1.1.13.1.4 or 1.2.840.10008.5.1.4.1.1.13.1.5) the isocenter coordinate system shall be used to describe the positioning of the X-Ray Source, Detector and Breast Support (see Section C.8.31.6), and shall use only the value ISOCENTER for Equipment Coordinate System Identification (0028,9537).

Prev | Up | Next
A.55.2 Breast Tomosynthesis Image IOD Entity-Relationship Model | Home | A.55.4 Breast Tomosynthesis Image Functional Group Macros

DICOM PS3.3 2018d - Information Object Definitions