DICOM PS3.3 2018d - Information Object Definitions

A.8.3 Multi-frame Grayscale Byte Secondary Capture Image IOD (Current)
Prev | A.8 Secondary Capture Image IOD | Next

### A.8.3 Multi-frame Grayscale Byte Secondary Capture Image IOD

#### A.8.3.1 Multi-frame Grayscale Byte Image IOD Description

The Multi-frame Grayscale Byte Secondary Capture (SC) Image Information Object Definition (IOD) specifies Grayscale Byte images that are converted from a non-DICOM format to a modality independent DICOM format.

This IOD is typically used for screen captured images for modalities that have pixel values of 8 bits, but may also be appropriate for scanned grayscale documents.

Prev | Up | Next
A.8.2.4 Multi-frame Single Bit SC Image IOD Content Constraints | Home | A.8.3.2 Multi-frame Grayscale Byte SC Image IOD Entity-Relationship Model

DICOM PS3.3 2018d - Information Object Definitions