DICOM PS3.3 2018d - Information Object Definitions

C.7.6.9 Frame Pointers Module (Current)
Prev | C.7.6 Common Image IE Modules | Next

#### C.7.6.9 Frame Pointers Module

Table C.7-15 specifies the Attributes of a Frame Pointer Module.

Table C.7-15. Frame Pointers Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Representative Frame Number | (0028,6010) | 3 | The frame number selected for use as a pictorial representation (e.g., icon) of the Multi-frame Image
Frame Numbers Of Interest (FOI) | (0028,6020) | 3 | Frame number(s) selected as frames of interest. A frame number may appear more than once.
Frame Of Interest Description | (0028,6022) | 3 | Description of each one of the Frame(s) of Interest selected in (0028,6020). If multiple Frames of Interest are selected and this Attribute is used, it shall contain the same number of values as are in Frame Numbers of Interest (0028,6020).
Frame of Interest Type | (0028,6023) | 3 | A Defined Term for each one of the Frame(s) of Interest (0028,6020) that identifies the significance of the frame. If multiple Frames of Interest are selected and this Attribute is used, it shall contain the same number of values as are in Frame Numbers of Interest (0028,6020). Defined Terms: HIGHMI a frame acquired at the time of the high power pulse that destroys acoustic contrast RWAVE the frame closest to the R-Wave TRIGGER a trigger frame, for example a set delay from the R Wave ENDSYSTOLE the frame closest to end of systole, at the end of the T-wave

### Note

1. Frame numbers begin at 1.

2. Frame of Interest Description is intended to indicate such frames as Systolic, Diastolic, Stenotic Artery, or trigger label.

Prev | Up | Next
C.7.6.8 Bi-plane Image Module (Retired) | Home | C.7.6.10 Mask Module

DICOM PS3.3 2018d - Information Object Definitions