DICOM PS3.17 2018d - Explanatory Information

EEEE.2 Encoding Diffusion Model Parameters for ROIs in Measurement Report SR Documents (Current)
Prev | EEEE Encoding Diffusion Model Parameters for Parametric Maps and ROI Measurements (Informative) | Next

## EEEE.2 Encoding Diffusion Model Parameters for ROIs in Measurement Report SR Documents

This example shows how to describe the mean ADC value of a region of interest on a volume of ADC values obtained from a pair of B0 and B1000 images fitting the log ratio ot two samples to a mono-exponential function (single compartment model). In this case the template used is TID 1419 “ROI Measurements”.

- NUM (113041, DCM, "Apparent Diffusion Coefficient") = 0.75E-3 (mm2/s, UCUM, "mm2/s")

  - HAS CONCEPT MOD CODE (G-C036, SRT, "Measurement Method") = (113250, DCM, "Mono-exponential ADC model")

  - HAS CONCEPT MOD CODE (113241, DCM, "Model fitting method") = (113260, DCM, "Log of ratio of two samples")

  - HAS CONCEPT MOD CODE (121401, DCM, "Derivation") = (R-00317, SRT, "Mean")

  - INFERRED FROM NUM (113240, DCM, "Source image diffusion b-value") = 0 (s/mm2, UCUM, "s/mm2")

  - INFERRED FROM NUM (113240, DCM, "Source image diffusion b-value") = 1000 (s/mm2, UCUM, "s/mm2")

  - HAS CONCEPT MOD TEXT (121050, DCM, "Equivalent Meaning of Concept Name") = "Mean ADC mono-exponential log ratio B0 and B1000"

Prev | Up | Next
EEEE Encoding Diffusion Model Parameters for Parametric Maps and ROI Measurements (Informative) | Home | EEEE.3 Relationship of Derived Diffusion Model Parametric Maps to Diffusion Weighted Source Images

DICOM PS3.17 2018d - Explanatory Information