DICOM PS3.3 2018d - Information Object Definitions

A.74.4 Breast Projection X-Ray Image Functional Group Macros (Current)
Prev | A.74 Breast Projection X-Ray Image IOD | Next

### A.74.4 Breast Projection X-Ray Image Functional Group Macros

Table A.74-2 specifies the use of the Functional Group Macros used in the Multi-frame Functional Groups Module for the Breast Projection X-Ray Image IOD.

Table A.74-2. Breast Projection X-Ray Image Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Frame Content | C.7.6.16.2.2 | M - May not be used as a Shared Functional Group.
Referenced Image | C.7.6.16.2.5 | U
Derivation Image | C.7.6.16.2.6 | C - Required if the Image Type (0008,0008) Value 1 equals DERIVED or Value 1 is ORIGINAL and Presentation Intent Type equals FOR PRESENTATION. May be present otherwise.
Frame Anatomy | C.7.6.16.2.8 | M
Identity Pixel Value Transformation | C.7.6.16.2.9b | M
Frame VOI LUT With LUT | C.7.6.16.2.10b | M
Contrast/Bolus Usage | C.7.6.16.2.12 | C - Required if the Enhanced Contrast/Bolus Module is present
Frame Display Shutter | C.7.6.16.2.16 | U
Irradiation Event Identification | C.7.6.16.2.18 | M
X-Ray Frame Characteristics | C.8.19.6.1 | U
X-Ray Field of View | C.8.19.6.2 | M
X-Ray Frame Pixel Data Properties | C.8.19.6.4 | M
X-Ray Frame Detector Parameters | C.8.19.6.5 | U
X-Ray Calibration Device Usage | C.8.19.6.6 | U
X-Ray Frame Acquisition | C.8.19.6.8 | U
X-Ray Collimator | C.8.19.6.12 | M
Breast X-Ray Positioner | C.8.31.2 | C - Required if X-Ray Source moves relative to the Patient. May be present otherwise.
Breast X-Ray Detector | C.8.31.3 | C - Required if X-Ray Detector plane is not normal to the X-Ray beam vector. May be present otherwise.
Breast X-Ray Geometry | C.8.31.4 | M
Breast X-Ray Acquisition Dose | C.8.31.5 | M
Breast X-Ray Isocenter Reference System | C.8.31.6 | M
X-Ray Grid | C.8.31.7 | U
X-Ray Filter | C.8.31.8 | U

#### A.74.4.1 Breast Projection X-Ray Image Functional Group Macros Content Constraints

##### A.74.4.1.1 Frame Anatomy Functional Group Macro

The Defined CID for the Anatomic Region Sequence (0008,2218) shall be CID 4013 “Anatomic Region for Mammography”.

Prev | Up | Next
A.74.3 Breast Projection X-Ray Image IOD Module Table | Home | A.75 Parametric Map IOD

DICOM PS3.3 2018d - Information Object Definitions