DICOM PS3.16 2018d - Content Mapping Resource

TID 4006 Mammography CAD Single Image Finding (Current)
Prev | Mammography CAD SR IOD Templates | Next

### TID 4006 Mammography CAD Single Image Finding

This Template describes a single image finding for a lesion or other object. The details of the finding are expressed in this Template and/or more specific Templates. The details from which a single image Calcification Cluster is inferred may be expressed in a number of Single Image Findings (see TID 4006 “Mammography CAD Single Image Finding”) of type Individual Calcification.

A Single Image Finding of type Breast Composition may be INFERRED FROM by-reference to a Single Image Finding of type Breast Geometry.

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4006. Mammography CAD Single Image Finding

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (111059, DCM, "Single Image Finding") | 1 | M |  | DCID 6014 “Mammography Single Image Finding”
2 | > | HAS CONCEPT MOD | CODE | EV (111056, DCM, "Rendering Intent") | 1 | M |  | DCID 6034 “Intended Use of CAD Output”
3 | >> | HAS PROPERTIES | NUM | EV (111071, DCM, "CAD Operating Point") | 1 | UC | IFF value of row 2 is (111151, DCM, "Presentation Optional") and row 9 of TID 4017 “CAD Detection Performed” is present | UNITS = DT ({1:n}, UCUM, "range: 1:n"), where n is the maximum specified in Row 9 of TID 4017 “CAD Detection Performed”. Value is restricted to being an integer
4 | > | HAS OBS CONTEXT | INCLUDE | DTID 4108 “Tracking Identifier” | 1 | U |  |
5 | > | HAS PROPERTIES | INCLUDE | DTID 4019 “Algorithm Identification” | 1 | M |  |
6 | > | HAS PROPERTIES | NUM | EV (111012, DCM, "Certainty of Finding") | 1 | U |  | UNITS = EV (%, UCUM, "Percent") Value = 0 - 100
7 | > | HAS PROPERTIES | NUM | EV (111047, DCM, "Probability of cancer") | 1 | UC | May be present unless value of parent is (F-01710, SRT, "Breast composition"), (111100, DCM, "Breast geometry"), (T-04100, SRT, "Nipple"), (111099, DCM, "Selected region"), (111101, DCM, "Image quality") or (111102, DCM, "Non-lesion") | UNITS = EV (%, UCUM, "Percent") Value = 0 - 100
8 | > | HAS PROPERTIES | INCLUDE | DTID 4021 “Mammography CAD Geometry” | 1 | MC | Shall be present unless value of parent is (F-01710, SRT, "Breast composition"), (111100, DCM, "Breast geometry") or (111101, DCM, "Image quality") |
9 | > | HAS PROPERTIES | INCLUDE | DTID 4007 “Mammography CAD Breast Composition” | 1 | MC | Shall be present only if value of parent is (F-01710, SRT, "Breast composition") |
10 | > | R-INFERRED FROM | CODE |  | 1-n | UC | May be present only if value of parent is (F-01710, SRT, "Breast composition") | Shall reference a (111059, DCM, "Single Image Finding") of value: EV (111100, DCM, "Breast geometry")
11 | > | HAS PROPERTIES | INCLUDE | DTID 4008 “Mammography CAD Breast Geometry” | 1 | MC | Shall be present only if value of parent is (111100, DCM, "Breast geometry") |
12 | > | HAS PROPERTIES | INCLUDE | DTID 4009 “Mammography CAD Individual Calcification” | 1 | UC | May be present only if value of parent is (F-01776, SRT, "Individual Calcification") |
13 | > | HAS PROPERTIES | INCLUDE | DTID 4010 “Mammography CAD Calcification Cluster” | 1 | UC | May be present only if value of parent is (F-01775, SRT, "Calcification Cluster") |
14 | > | HAS PROPERTIES | INCLUDE | DTID 4011 “Mammography CAD Density” | 1 | UC | May be present only if value of parent is (F-01796, SRT, "Mammography breast density") |
15 | > | HAS PROPERTIES | CODE | EV (111297, DCM, "Nipple Characteristic") | 1 | UC | May be present only if value of parent is (T-04100, SRT, "Nipple") | DCID 6039 “Nipple Characteristic”
16 | > | HAS PROPERTIES | INCLUDE | DTID 4012 “Mammography CAD Non-lesion” | 1 | MC | Shall be present only if value of parent is (111102, DCM, "Non-lesion") |
17 | > | HAS PROPERTIES | INCLUDE | DTID 4013 “Mammography CAD Selected Region” | 1 | MC | Shall be present only if value of parent is (111099, DCM, "Selected Region") |
18 | > | R-INFERRED FROM | IMAGE |  | 1 | MC | IF value of parent is (111101, DCM, "Image quality") and IFF row 19 is not present | Shall reference an IMAGE Content Item in the (111028, DCM, "Image Library")
19 | > | HAS PROPERTIES | SCOORD | EV (111030, DCM, "Image Region") | 1-n | MC | IF value of parent is (111101, DCM, "Image quality") and IFF row 18 is not present |
20 | >> | R-SELECTED FROM | IMAGE |  | 1 | M |  | All the (111030, DCM, "Image Region") Content Items in a single invocation of this Template shall reference the same IMAGE Content Item in the (111028, DCM, "Image Library")
21 | > | HAS PROPERTIES | INCLUDE | DTID 4014 “CAD Image Quality” | 1-n | MC | Shall be present only if value of parent is (111101, DCM, "Image quality") | $QualityFinding = DCID 6041 “Mammography Image Quality Finding” $QualityStandard = DCID 6045 “Mammography Types of Quality Control Standard”
22 | > | HAS PROPERTIES | NUM | DCID 6142 “Calculated Value” | 1-n | U |  |
23 | >> | HAS CONCEPT MOD | CODE | EV (121401, DCM, "Derivation") | 1 | M |  | DCID 6140 “Calculation Methods”
24 | >> | INFERRED FROM | TEXT | EV (112034, DCM, "Calculation Description") | 1 | U |  |
25 | > | INFERRED FROM | INCLUDE | DTID 4006 “Mammography CAD Single Image Finding” | 1-n | UC | May be present only if value of parent is (F-01775, SRT, "Calcification Cluster") | EV (F-01776, SRT, "Individual Calcification")
26 | > | HAS OBS CONTEXT | INCLUDE | DTID 4022 “CAD Observation Context” | 1 | MC | Shall be present only if this finding is incorporated from a different report than its parent. |

Content Item Descriptions

Rendering Intent | This Content Item constrains the SCP receiving the Mammography CAD SR IOD in its use of the contents of this Template and its Target Content Items. Mammography CAD devices may opt to use data marked "Not for Presentation" or "Presentation Optional" as input to subsequent mammography CAD processing steps. Refer to Section O.2 “Structured Reporting Storage SOP Class SCU and SCP Behavior” in PS3.4 .
CAD Operating Point | Additional information to use when Rendering Intent is "Presentation Optional". A CAD Operating Point of zero is not sent, and is encoded as a Rendering Intent of "Presentation Required". See Section O.2 “Structured Reporting Storage SOP Class SCU and SCP Behavior” in PS3.4 and Section E.4 “CAD Operating Point” in PS3.17 .
Single Image Finding | A Single Image Finding (whose parent is a Single Image Finding of type Calcification Cluster) allows one level of nesting for the definition of individual calcifications within the cluster. To use this Template recursively, this Single Image Finding code value shall be "Individual Calcification".
Certainty of Finding | The likelihood that the finding detected, and classified by the CODE specified in the Single Image Finding parent Template, is in fact that type of finding.

Prev | Up | Next
TID 4005 Mammography CAD Composite Feature Body | Home | TID 4007 Mammography CAD Breast Composition

DICOM PS3.16 2018d - Content Mapping Resource