DICOM PS3.17 2018d - Explanatory Information

C.6.3 Timing (Current)
Prev | C.6 Harmonization With HL7 | Next

### C.6.3 Timing

In HL7, the exact start time for waveform data is sent in an OBX Segment of subtype TIM. The corresponding DICOM attributes, which must be combined to form the equivalent time string, are:

Acquisition DateTime | (0008,002A)
Multiplex Group Time Offset | (0018,1068)

Prev | Up | Next
C.6.2 Channel Definition | Home | C.6.4 Waveform Data

DICOM PS3.17 2018d - Explanatory Information