DICOM PS3.2 2018d - Conformance

F.4.4 Configuration (Current)
Prev | F.4 Networking | Next

### F.4.4 Configuration

#### F.4.4.1 AE Title/Presentation Address Mapping

##### F.4.4.1.1 Local AE Titles

The mapping from AE Title to TCP/IP addresses and ports is configurable and set at the time of installation by Installation Personnel.

Table F.4.4-1. Default Application Entity Characteristics

Application Entity | Role | Default AE Title | Default TCP/IP Port
--- | --- | --- | ---
STORAGE-SCU | SCU | EX_STORE_SCU | None
STORAGE-SCP | SCP | EX_STORE_SCP | 4000
QUERY-RETRIEVE-SCP | SCP | EX_QUERY_SCP | 5000

The STORAGE-SCU and QUERY-RETRIEVE-SCP Application Entities can be configured to have the same AE Title. The STORAGE-SCP Application Entity must not have the same AE Title as the other two.

##### F.4.4.1.2 Remote AE Title/Presentation Address Mapping

The mapping of external AE Titles to TCP/IP addresses and ports is configurable and set at the time of installation by Installation Personnel. This mapping is necessary for resolving the IP address and port of C-MOVE Destination Application Entities and must be correctly configured for the QUERY-RETRIEVE-SCP AE to correctly function as a C-MOVE SCP.

Prev | Up | Next
F.4.3.3 IPv4 and IPv6 Support | Home | F.4.4.2 Parameters

DICOM PS3.2 2018d - Conformance