DICOM PS3.3 2018d - Information Object Definitions

A.83 Ophthalmic Optical Coherence Tomography En Face Image Information Object Definition (Current)
Prev | A Composite Information Object Definitions (Normative) | Next

## A.83 Ophthalmic Optical Coherence Tomography En Face Image Information Object Definition

This Section defines an Information Object to be used with several types of en face images that are derived from volumetric images obtained using OCT technology. En face images may be based upon structural OCT volumes and surface mesh information only or structural OCT volumes, surface mesh information and angiographic flow volume information.

### A.83.1 Ophthalmic Optical Coherence Tomography En Face Image IOD Description

The Ophthalmic Optical Coherence Tomography En Face Image IOD specifies a single-frame image derived from images obtained using OCT technology. This IOD encodes a single derived en face image.

Prev | Up | Next
A.82.3 Protocol Approval Information Object Definitions | Home | A.83.2 Ophthalmic Optical Coherence Tomography En Face Image IOD Entity-Relationship Model

DICOM PS3.3 2018d - Information Object Definitions