DICOM PS3.11 2018d - Media Storage Application Profiles

M.3.4 Other Parameters (Current)
Prev | M.3 STD-GEN-BD and STD-GEN-SEC-BD Profile Classes | Next

### M.3.4 Other Parameters

#### M.3.4.1 Multi-frame JPEG Format

The JPEG encoding of pixel data shall use Interchange Format (with table specification) for all frames.

Prev | Up | Next
M.3.3 Directory Information in DICOMDIR | Home | M.3.5 Security Parameters

DICOM PS3.11 2018d - Media Storage Application Profiles