DICOM PS3.2 2018d - Conformance

D.5.2 AE Specifications (Current)
Prev | D.5 Media Interchange | Next

### D.5.2 AE Specifications

#### D.5.2.1 MEDIA-FSR

MEDIA-FSR provides standard conformance to the Media Storage Service Class.

Table D.5.2-1. Application Profiles, Activities, and Roles for MEDIA-FSR

Application Profiles Supported | Real World Activity | Role
--- | --- | ---
STD-GEN-CD | Load directory or file | FSR
STD-GEN-DVD-RAM | Load directory or file | FSR

### Note

The application is media neutral and dependent on the underlying hardware. Any (non-secure) General Purpose Profile can be supported.

##### D.5.2.1.1 File Meta Information for the Application Entity

Not applicable, since MEDIA-FSR is not an FSC or FSU.

##### D.5.2.1.2 Real World Activities

###### D.5.2.1.2.1 Activity - Load Directory or File

MEDIA-FSR is activated through the user interface when a user selects the File load operation.

If the loaded file is a DICOMDIR, a browser will be displayed, from which instances may be selected and in turn loaded for display, imported into the local database or sent to a remote AE over the network.

If the file is an image or spectroscopy instance, it will be loaded and displayed.

###### D.5.2.1.2.1.1 Application Profile Specific Conformance

There are no extensions or specializations.

Prev | Up | Next
D.5 Media Interchange | Home | D.5.3 Augmented and Private Profiles

DICOM PS3.2 2018d - Conformance