DICOM PS3.2 2018d - Conformance

E.8 Annexes (Current)
Prev | E Conformance Statement Example Print Server (Informative) | Next

## E.8 Annexes

### E.8.1 IOD Contents

#### E.8.1.1 Created IOD Instance(s)

The EXAMPLE-PRINT-SERVER-MANAGEMENT creates the following IOD types of instances: Image Boxes, Annotation Boxes, Print Jobs, Printer, and Printer Configuration.

The attributes of the created IODs are described in the SOP Specific Conformance, Section E.4.2.1.4.1.3.

#### E.8.1.2 Usage of Attributes From Received IODs

The usage of attributes received in the IODs sent by the Print SCU is described in the SOP Specific Conformance, Section E.4.2.1.4.1.3.

#### E.8.1.3 Attribute Mapping

The following table is a mapping table of attributes that can be set by different Print IODs. If more then one IOD is setting the same element, then the value will be over-written by the IOD's value in the order from left to right, such that the Printer Configuration (PC) specific element values (as described in the mapping table #45) is in lowest order might be overwritten by any other IOD.

Table E.8.1-1. Print Server Attribute Mapping

Attribute Name | Tag | PC | FS | FB | IB | PI | PJ
--- | --- | --- | --- | --- | --- | --- | ---
Print Priority | (2000,0020) |  | X |  |  |  | X
Medium Type | (2000,0030) | X | X |  |  |  |
Image Display Format | (2010,0010) | X |  | X | X |  |
Film Orientation | (2010,0040) | X |  | X |  |  |
Film Size ID | (2010,0050) | X |  | X |  |  |
Magnification Type | (2010,0060) |  |  | X | X |  |
Smoothing Type | (2010,0080) |  |  | X | X |  |
Min Density | (2010,0120) | X |  | X |  |  |
Max Density | (2010,0130) | X |  | X |  |  |
Configuration Information | (2010,0150) |  |  | X | X |  |
Printer Name | (2110,0030) |  |  |  |  | X | X

Print Management IODs Abbreviations

PC - Printer Configuration

FS - Film Session

FB - Film Box

IB - Image Box

PI - Printer Information

PJ - Print Job

The IODs in the above table are in the order from Left to Right over-writing values that are already set by previous IODs. For Example: the Print Priority element can be set by both the Film Session and the Print Job, however if both IODs are setting this values then the Print Job Print Priority value will over write the Film Session Print Priority value.

#### E.8.1.4 Coerced/Modified Fields

The EXAMPLE-PRINT-SERVER-MANAGEMENT AE will truncate attribute values received from the Print Composer (SCU) if the value length is longer than the maximum length permitted by the attribute VR.

Prev | Up | Next
E.7 Security | Home | E.8.2 Data Dictionary of Private Attributes

DICOM PS3.2 2018d - Conformance