DICOM PS3.17 2018d - Explanatory Information

EEE.2 IVOCT For Processing Parameters (Current)
Prev | EEE Intravascular OCT Image (Informative) | Next

## EEE.2 IVOCT For Processing Parameters

### EEE.2.1 Z Offset Correction

When an OCT image is acquired, the path length difference between the reference and sample arms may vary, resulting in a shift along the axial direction of the image, known as the Z Offset. With FOR PROCESSING images, in order to convert the image in Cartesian coordinates and make measurements, this Z Offset should be corrected, typically on a per-frame or per-image basis. Z Offset is corrected by shifting Polar data rows (A-lines) + OCT Z Offset Correction (0052,0030) pixels along the axial dimension of the image.

Z Offset correction may be either a positive or negative value. Positive values mean that the A-lines are shifted further away from the catheter optics. Negative values mean that the A-lines are shifted closer to the catheter optics. Figure EEE.2-1 illustrates a negative Z Offset Correction.

Figure EEE.2-1. Z Offset Correction

Prev | Up | Next
EEE Intravascular OCT Image (Informative) | Home | EEE.2.2 Refractive Index Correction

DICOM PS3.17 2018d - Explanatory Information