DICOM PS3.7 2018d - Message Exchange

A.6 Association Abort for DICOM AE (Current)
Prev | A Application Context Usage (Normative) | Next

## A.6 Association Abort for DICOM AE

Either DICOM AE may initiate an abrupt termination of an Association. This shall be accomplished by using the A-ABORT service defined in PS3.8.

Upon receiving or issuing the A-ABORT service primitive, the DICOM AE Association-requester and DICOM AE Association-acceptor shall fail any operation that is outstanding.

### Note

The Association services and presentation services defined in the Upper Layer Service in PS3.8 are a fully conformant subset of the services offered by the ACSE and the OSI Presentation Layer.

Prev | Up | Next
A.5 Association Release for DICOM AE | Home | B Index to Application Context Name UIDs (Informative)

DICOM PS3.7 2018d - Message Exchange