DICOM PS3.4 2018d - Service Class Specifications

FF.2.5 Display Layout (Current)
Prev | FF.2.4 Additional Volumetric Considerations | Next

#### FF.2.5 Display Layout

The layout of multiple Volumetric Presentation States is not specified by the Volumetric Transformation process. However, there are attributes within Volumetric Presentation States that can influence the overall display layout.

For instance:

- Anatomic Region Sequence (0008,2218) specifies the anatomic region covered by the Volumetric Presentation State

- View Code Sequence (0054,0220) describes the view of the anatomic region of interest (e.g., Coronal, Oblique transverse, etc.)

- Presentation Display Collection UID (0070,1101) identifies the Presentation State as one of a set of views intended to be displayed together

- SOP Class UID (0008,0016) identifies that the Presentation State describes the volumetric view

The use of these attributes allows a display application to create an appropriate presentation of multiple Volumetric Presentation States, whether through the application of a Hanging Protocol instance, a Structured Display instance or by means of an application-specific algorithm.

For an example of their use, see Annex XXX “Volumetric Presentation States (Informative)” in PS3.17.

Prev | Up | Next
FF.2.4.2.5 Swivel Animation | Home | FF.3 Behavior of An SCP

DICOM PS3.4 2018d - Service Class Specifications