DICOM PS3.3 2018d - Information Object Definitions

A.52 Ophthalmic Tomography Image IOD (Current)
Prev | A Composite Information Object Definitions (Normative) | Next

## A.52 Ophthalmic Tomography Image IOD

This Section defines an Information Object to be used with optical ophthalmic tomographic imaging devices, including optical coherence scanners and confocal scanning laser ophthalmoscopes, but excluding ophthalmic ultrasound devices.

### A.52.1 Ophthalmic Tomography Image IOD Description

The Ophthalmic Tomography Image IOD specifies a single-frame or a multi-frame image acquired on an Ophthalmic Tomography modality. This IOD can be used to encode both single and multi-frame ophthalmic images.

Prev | Up | Next
A.51.5 Segmentation Functional Groups | Home | A.52.2 Ophthalmic Tomography Image IOD Entity-Relationship Model

DICOM PS3.3 2018d - Information Object Definitions