DICOM PS3.3 2018d - Information Object Definitions

A.84.3.2 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis Functional Group Macros (Current)
Prev | A.84.3 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis IOD Modules | Next

#### A.84.3.2 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis Functional Group Macros

Table A.84.3.2-1 specifies the use of the Functional Group Macros used in the Multi-frame Functional Groups Modulefor the Ophthalmic Optical Coherence Tomography B-scan Volume Analysis IOD.

Table A.84.3.2-1. Ophthalmic Optical Coherence Tomography B-scan Volume Analysis Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Pixel Measures | C.7.6.16.2.1 | M
Plane Orientation (Patient) | C.7.6.16.2.4 | M
Plane Position (Patient) | C.7.6.16.2.3 | M
Frame Content | C.7.6.16.2.2 | M - May not be used as a Shared Functional Group.
Referenced Image | C.7.6.16.2.5 | M
Derivation Image | C.7.6.16.2.6 | M - May not be used as a Shared Functional Group (see Section A.84.3.2.1.1 for specialization).
Frame Anatomy | C.7.6.16.2.8 | M
Frame VOI LUT With LUT Macro | C.7.6.16.2.10b | M
Real World Value Mapping | C.7.6.16.2.11 | U

##### A.84.3.2.1 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis IOD Content Constraints

This source for an Ophthalmic Optical Coherence Tomography B-scan Volume Analysis SOP Instance is one or more multi-frame Ophthalmic Tomography SOP Instance(s). The correlation is encoded at the Frame Level and conveyed in the Derivation Image Macro (see Section C.8.17.14.1.7 for examples).

###### A.84.3.2.1.1 Derivation Image Functional Group

The following constraints to the Derivation Image Macro shall apply:

1. Derivation Image Sequence (0008,9124) shall be Type 1

2. The value for Derivation Code Sequence (0008,9215) shall be (128303, DCM, "OCT B-scan analysis")

3. Source Image Sequence (0008,2112) shall be Type 1 and contain one Item. The referenced SOP Instance shall have the same value for Frame of Reference UID (0020,0052) as this SOP Instance

4. The value for Referenced SOP Class UID (0008,1150) shall be Ophthalmic Tomography Image Storage ("1.2.840.10008.5.1.4.1.1.77.1.5.4")

5. The value for Purpose of Reference Code Sequence (0040,A170) shall be (128250, DCM, "Structural image for imaging processing")

6. The value for Spatial Locations Preserved (0028,135A) shall be YES

Prev | Up | Next
A.84.3 Ophthalmic Optical Coherence Tomography B-scan Volume Analysis IOD Modules | Home | A.85 Encapsulated 3D Manufacturing Model IODs

DICOM PS3.3 2018d - Information Object Definitions