DICOM PS3.3 2018d - Information Object Definitions

A.60.6 Ophthalmic Axial Measurements IOD (Current)
Prev | A.60 Ophthalmic Refractive Measurements Information Object Definitions | Next

### A.60.6 Ophthalmic Axial Measurements IOD

#### A.60.6.1 Ophthalmic Axial Measurements IOD Description

The Ophthalmic Axial Measurements IOD is used to encode axial measurements of the eye made by an axial measurements device.

Prev | Up | Next
A.60.5.3 Visual Acuity Measurements IOD Module Table | Home | A.60.6.2 Ophthalmic Axial Measurements IOD Entity-Relationship Model

DICOM PS3.3 2018d - Information Object Definitions