DICOM PS3.4 2018e - Service Class Specifications

DD.3.2.3.2 Status (Current)
Prev | DD.3.2.3 N-ACTION | Next

##### DD.3.2.3.2 Status

Table DD.3.2.3-2 defines the status code values that might be returned in a N-ACTION response. General status code values and fields related to status code values are defined for N-ACTION DIMSE Service in PS3.7.

Table DD.3.2.3-2. RT Conventional Machine and RT Ion Machine Verification SOP Class N-ACTION Status Values

Service Status | Further Meaning | Status Code
--- | --- | ---
Success | Machine Parameter Verification of the applicable Machine Verification instance successfully initiated. | 0000
Failure | Failed; Machine Verification requested instance not found. | C112

Prev | Up | Next
DD.3.2.3 N-ACTION | Home | DD.3.2.3.3 Behavior

DICOM PS3.4 2018e - Service Class Specifications