DICOM PS3.3 2018e - Information Object Definitions

C.11.27.5 Use of Segmented Palette Color Lookup Tables (Current)
Prev | C.11.27 MPR Volumetric Presentation State Display Module | Next

#### C.11.27.5 Use of Segmented Palette Color Lookup Tables

Segmented Palette Color Lookup Tables provide a means for specifying lookup tables in a parametric manner rather than as a set of discrete mapping values.

### Note

Specifying tables using the segmented method may be preferred by color mapping implementations based on control points.

The value of Segmented Alpha Palette Color Lookup Table (0028,1224) is structured in the same manner as Segmented Red Palette Color Lookup Table Data (0028,1221), Segmented Green Palette Color Lookup Table Data (0028,1222), and Segmented Blue Palette Color Lookup Table Data (0028,1221) described in Section C.7.9.2 “Segmented Palette Color Lookup Table Data”.

Prev | Up | Next
C.11.27.4 Weighting Transfer Function | Home | C.11.28 Volumetric Graphic Annotation Module

DICOM PS3.3 2018e - Information Object Definitions