DICOM PS3.4 2018e - Service Class Specifications

EE.2.4 Reserved Identifications (Current)
Prev | EE.2 Display System SOP Class | Next

### EE.2.4 Reserved Identifications

The well-known UID of the Display System SOP Instance shall have the value of "1.2.840.10008.5.1.1.40.1".

Prev | Up | Next
EE.2.3 SOP Class Definitions and UIDs | Home | EE.3 Conformance

DICOM PS3.4 2018e - Service Class Specifications