DICOM PS3.17 2018e - Explanatory Information

IIII.2 Example of Fused CT/MR Derived Encapsulated STL (Current)
Prev | IIII Encapsulated STL (Informative) | Next

## IIII.2 Example of Fused CT/MR Derived Encapsulated STL

In this example, the patient will shortly be undergoing a complex cardiac surgery. A 3D manufacturing model (encoded in binary STL) was created to manufacture a surgical planning aid representing the patient's unique anatomy.

To begin, a series of CT images (CT-02) and a series of MR images (MR-01) were registered using CT-02's frame of reference as the base coordinate system and then fused. An initial version of the model was derived and reviewed by the surgical team who requested that some of the anatomy surrounding the heart be removed. A second version of the model was created on July 16, 2017 at 1:04:34 PM then stored in a DICOM instance at 1:33:01 PM. The CT and MR data were acquired at earlier dates.

The Encapsulated STL file shown in this example is the second version..

Both versions of the STL were created in the coordinate system of CT-02; so they all share the same Frame of Reference value.

Note: Mapping to other Frames of Reference of secondary source series would be handled via registration objects.

A preview image (optional) showing the rendered 3D object was created and included with the encapsulated STL as an icon image.

The creator of the model inscribed the patient's medical record number on a side of the model to avoid the possibility of a wrong patient error.

Table IIII.2-1. Fused CT/MR Derived Encapsulated STL Example

Attribute Name | Tag | Example Value | Comments
--- | --- | --- | ---
<Patient and General Study Modules not shown for brevity>
Modality | (0008,0060) | M3D |
Series Instance UID | (0020,000E) | 2.999.89235.5951.35894.0086 |
Series Number | (0020,0011) | 6 |
Series Description | (0008,103E) | 3DP Models |
Instance Number | (0020,0013) | 2 |
Frame of Reference UID | (0020,0052) | 1.2.3.4.5.6.777.0.1 |
Manufacturer | (0008,0070) | Acme Additive Inc |
Manufacturer's Model Name | (0008,1090) | Cardioplan |
Device Serial Number | (0018,1000) | 10065789 |
Software Versions | (0018,1020) | 6.3 |
Content Date | (0008,0023) | 20170716 |
Content Time | (0008,0033) | 130034 |
Acquisition DateTime | (0008,002A) | 20170716130034 |
Image Laterality | (0020,0062) | U |
Burned In Annotation | (0028,0301) | YES |
Recognizable Visual Features | (0028,0302) | NO |
Source Instance Sequence | (0042,0013) |  | A sequence referencing CT-02 and MR-01 source images because both were used.
%item |  |  |
>Referenced SOP Class UID | (0008,1150) | 1.2.840.10008.5.1.4.1.1.2.1 | Referenced object is an Enhanced CT Image Storage Instance
>Referenced SOP Instance UID | (0008,1155) | 2.999.89235.5951.35894.153 | The multi-frame CT instance from study CT-02
>Purpose of Reference Code Sequence | (0040,A170) | (121324, DCM, "Source image") | CID 7060 “Encapsulated Document Source Purposes of Reference”
%enditem |  |  |
%item |  |  |
>Referenced SOP Class UID | (0008,1150) | 1.2.840.10008.5.1.4.1.1.4.1 | Referenced object is an Enhanced MR Image Storage Instance
>Referenced SOP Instance UID | (0008,1155) | 2.999.89235.5951.35894.154 | The multi-frame MR instance from study MR-01
>Purpose of Reference Code Sequence | (0040,A170) | (121324, DCM, "Source image") | CID 7060 “Encapsulated Document Source Purposes of Reference”
%enditem |  |  |
Document Title | (0042,0010) | Mixed Modality 3D CAM model |
Concept Name Code Sequence | (0040,A043) | (129019, DCM, "Mixed Modality 3D CAM model") | CID 7061 “Model Document Titles”
Predecessor Documents Sequence | (0040,A360) |  | A reference to the earlier encapsulated STL
%item |  |  |
>Study Instance UID | (0020,000D) | 2.999.1241.1515.15151.515.62 |
>Reference Series Sequence | (0008,1115) |  |
%item |  |  |
>>Series Instance UID | (0020,000E) | 2.999.89235.5951.35894.151 |
>>Referenced SOP Sequence | (0008,1199) |  |
%item |  |  |
>>>Referenced SOP Class UID | (0008,1150) | 1.2.840.10008.5.1.4.1.1.104.3x | Encapsulated STL SOP Class
>>>Referenced SOP Instance UID | (0008,1155) | 2.999.1241.1515.15151.515.68 |
%enditem |  |  |
>>Purpose of Reference Code Sequence | (0040,A170) | (129010, DCM, "Edited Model") | CID 7062 “Purpose of Reference to Predecessor 3D Model”
%enditem |  |  |
%enditem |  |  |
MIME Type of Encapsulated Document | (0040,0012) | model/stl |
Encapsulated Document | (0042,0011) | <Byte stream representing the binary STL file> | Note that ASCII STL files are not supported.
Content Description | (0070,0081) | Pre-surgery cardiac model from CT and MR |
Measurement Units Code Sequence | (0040,08EA) | (mm, UCUM, "mm") |
Model Modification | (0068,7001) | NO |
Model Mirroring | (0068,7002) | NO |
Model Usage Code Sequence | (0068,7003) | (129013, DCM, "Planning Intent") | CID 7064 “Model Usage” In this example, the goal is to help plan the surgery, so the value is "Planning Intent".
Icon Image Sequence | (0088,0200) |  | Sequence containing the pre-rendered preview image
%item |  |  |
<Content of Table C.7-11b "Image Pixel Macro Attributes" not shown>
%enditem |  |  |
SOP Class UID | (0008,0016) | 1.2.840.10008.5.1.4.1.1.104.3 |
SOP Instance UID | (0008,0018) | 2.999.1241.1515.15151.515.987 |
Instance Creation Date | (0008,0012) | 20170716 |
Instance Creation Time | (0008,0013) | 133301 |

Prev | Up | Next
IIII Encapsulated STL (Informative) | Home | JJJJ Multi-energy CT Imaging (Informative)

DICOM PS3.17 2018e - Explanatory Information