DICOM PS3.4 2018e - Service Class Specifications

H.4.2 Basic Film Box SOP Class (Current)
Prev | H.4 Print Management SOP Class Definitions | Next

### H.4.2 Basic Film Box SOP Class

#### H.4.2.1 IOD Description

The Basic Film Box IOD is an abstraction of the presentation of one film of the film session. The Basic Film Box IOD describes the presentation parameters that are common for all images on a given sheet of film.

The Basic Film Box SOP Instance refers to one or more Image Box SOP Instances, zero or more film related Annotation Box SOP Instances, and zero or one Presentation LUT SOP Instance.

Prev | Up | Next
H.4 Print Management SOP Class Definitions | Home | H.4.2.2 DIMSE Service Group

DICOM PS3.4 2018e - Service Class Specifications