DICOM PS3.4 2018e - Service Class Specifications

P.2.2.4 Status Codes (Current)
Prev | P.2.2 Operation | Next

#### P.2.2.4 Status Codes

Table P.2-3 defines the specific status code values that might be returned in a N-ACTION response. See PS3.7 for additional general response status codes.

Table P.2-3. Response Status

Service Status | Further Meaning | Status Code
--- | --- | ---
Success |  | 0000
Warning | Specified Synchronization Frame of Reference UID does not match SCP Synchronization Frame of Reference | B101
Warning | Study Instance UID coercion; Event logged under a different Study Instance UID | B102
Warning | IDs inconsistent in matching a current study; Event logged | B104
Failure | Failed: Procedural Logging not available for specified Study Instance UID | C101
Failure | Failed: Event Information does not match Template | C102
Failure | Failed: Cannot match event to a current study | C103
Failure | Failed: IDs inconsistent in matching a current study; Event not logged | C104

Prev | Up | Next
P.2.2.3 Service Class Provider Behavior | Home | P.2.2.5 Action Reply

DICOM PS3.4 2018e - Service Class Specifications