DICOM PS3.8 2018e - Network Communication Support for Message Exchange

7.4.2 A-P-ABORT Service Procedure (Current)
Prev | 7.4 A-P-ABORT Service | Next

### 7.4.2 A-P-ABORT Service Procedure

When the UL service-provider detects an internal error, A-P-ABORT indication primitives shall be issued to acceptors in both AEs. The association shall be abnormally released. Requestors in both AEs shall not issue any further primitives for the association.

Prev | Up | Next
7.4 A-P-ABORT Service | Home | 7.5 Sequencing Information

DICOM PS3.8 2018e - Network Communication Support for Message Exchange