DICOM PS3.18 2018e - Web Services

8.2.5 Windowing (Current)
Prev | 8.2 Parameters for DICOM Images | Next

### 8.2.5 Windowing

The Windowing parameters are optional; however, if either is present, both shall be present. If only one is present the origin server shall return a 400 (Bad Request) response, and may include a payload containing an appropriate error message.

The Windowing and Presentation State parameters shall not be present in the same request. If both are present the origin server shall return a 400 (Bad Request) response, and may include a payload containing an appropriate error message.

The Windowing parameters shall not be present if contentType is application/dicom; if either is present the origin server shall return a 400 (Bad Request) response, and may include a payload containing an appropriate error message.

#### 8.2.5.1 Window Center of the Image

The parameter name shall be "windowCenter" for URI mode.

It controls the window center of the images as defined in PS3.3. This parameter is OPTIONAL for the URI mode.

The value shall be encoded as a decimal string (DS), as specified in PS3.5.

Prev | Up | Next
8.2.4 Region of the Image | Home | 8.2.5.2 Window Width of the Image

DICOM PS3.18 2018e - Web Services