DICOM PS3.17 2018e - Explanatory Information

FFF.2.3.3.4 Examples (Current)
Prev | FFF.2.3.3 Pixel-shift | Next

##### FFF.2.3.3.4 Examples

###### FFF.2.3.3.4.1 Usage of Pixel Shift Macro in Shared Context

In this example, the pixel shift -0.3\2.0 is applied to the frames 2 and 3 when they are subtracted to the mask frame 1 as defined in the Mask Subtraction Sequence.

Figure FFF.2.3-3. Example of Shared Frame Pixel Shift Macro

###### FFF.2.3.3.4.2 Usage of Pixel Shift Macro in "per Frame" Context

The usage in a per-frame context is expected in a typical clinical scenario where the shift between the mask and the contrast frames is not constant across the frames of the multi-frame image to compensate for patient/organ movement.

The encoded values of the key attributes of this example are shown in Figure FFF.2.3-4.

Figure FFF.2.3-4. Example of Per-Frame Frame Pixel Shift Macro

###### FFF.2.3.3.4.3 Usage of Pixel Shift Macro in "per Frame" Context For Multiple Shifts

The usage in a per-frame context is also appropriate to specify more than one set of shifts in case of more than one region of interest suffered from patient/organ movement independently, like in case of the two legs imaged simultaneously.

In this example, two Subtraction Item IDs are defined in the Mask Subtraction Sequence.

The encoded values of the key attributes of this example are shown in Figure FFF.2.3-5.

Figure FFF.2.3-5. Example of Per-Frame Frame Pixel Shift Macro for Multiple Shifts

Prev | Up | Next
FFF.2.3.3.3 Encoding Details | Home | FFF.2.4 Processing

DICOM PS3.17 2018e - Explanatory Information