DICOM PS3.4 2018e - Service Class Specifications

3.10 Device Independent Pixel Values (Current)
Prev | 3 Definitions | Next

## 3.10 Device Independent Pixel Values

This Part of the Standard makes use of the following terms defined in PS3.3:

1. P-Value

2. PCS-Value

Prev | Up | Next
3.9 DICOM Service Class Definitions | Home | 3.11 HTTP Definitions

DICOM PS3.4 2018e - Service Class Specifications