DICOM PS3.3 2018e - Information Object Definitions

A.60.2 Autorefraction Measurements IOD (Current)
Prev | A.60 Ophthalmic Refractive Measurements Information Object Definitions | Next

### A.60.2 Autorefraction Measurements IOD

#### A.60.2.1 Autorefraction Measurements IOD Description

The Autorefraction Measurements IOD is used to encode the results of a modality (autorefractor) that automatically determines, without Patient input, what a Patient's refractive correction should be.

Prev | Up | Next
A.60 Ophthalmic Refractive Measurements Information Object Definitions | Home | A.60.2.2 Autorefraction Measurements IOD Entity-Relationship Model

DICOM PS3.3 2018e - Information Object Definitions