DICOM PS3.3 2018e - Information Object Definitions

C.10.6 Spatial Transformation Module (Current)
Prev | C.10 Curve, Graphic and Waveform | Next

### C.10.6 Spatial Transformation Module

This Module defines a manner of rotating an image by increments of ninety degrees and flipping an image.

Table C.10-6. Spatial Transformation Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Image Rotation | (0070,0042) | 1 | How far to rotate the image clockwise in degrees, before any Image Horizontal Flip (0070,0041) is applied. Enumerated Values: 270 180 90 0 ### Note Negative values are not permitted since the Value Representation is unsigned.
Image Horizontal Flip | (0070,0041) | 1 | Whether or not to flip the image horizontally after any Image Rotation has been applied such that the left side of the image becomes the right side. Enumerated Values: Y yes N no ### Note No vertical flip is specified since the same result can be achieved by a combination of a 180 degree rotation and a horizontal flip.

### Note

Given the definition of the Grayscale Transformation Sequence in PS3.4, it is apparent that the rotation, flipping and magnification will be applied AFTER the application of any bit-mapped overlays or graphic annotations that are specified in the image pixel spaces, but BEFORE the application of graphic annotations that apply in the Specified Displayed Area relative space.

Prev | Up | Next
C.10.5 Graphic Annotation Module | Home | C.10.7 Graphic Layer Module

DICOM PS3.3 2018e - Information Object Definitions