DICOM PS3.18 2018e - Web Services

6.9.3 SearchForUPS (Current)
Prev | 6.9 UPS-RS Worklist Service | Next

### 6.9.3 SearchForUPS

This resource returns a list of UPS Instances that match specified search query parameters along with requested attributes for each Instance.

#### 6.9.3.1 Request

The request message shall be formed as follows:

- Resource

  - {+SERVICE}/workitems/{?query*}

    where

    - {+SERVICE} is the base URL for the service. This may be a combination of protocol (either HTTP or HTTPS), authority and path.

- Method

  - GET

- Headers

  - Accept - The representation scheme in which the RESTful service is requested to return the results. The types allowed for this request header are as follows:

    - multipart/related; type="application/dicom+xml"; boundary={messageBoundary}

      Specifies that the results should be DICOM PS3.19 XML metadata.

    - application/dicom+json

      Specifies that the results should be DICOM PS3.18 JSON metadata.

  - Cache-control: no-cache (recommended)

    If included, specifies that search results returned should be current and not cached.

- {query}

  - {attributeID}={value}

    0-n / {attributeID}={value} pairs allowed

  - includefield={attributeID} | all

    0-n includefield / {attributeID} pairs allowed, where "all" indicates that all attributes with values should be included for each response.

    Each {attributeID} shall refer to an attribute of the Unified Procedure Step IOD (see Section B.26.2 in PS3.3 ).

    See Section 6.7.1.1 for {attributeID} and {value} encoding rules

  - fuzzymatching=true | false

  - limit={maximumResults}

  - offset={skippedResults}

Prev | Up | Next
6.9.2.3.3 Response Message Body | Home | 6.9.3.2 Behavior

DICOM PS3.18 2018e - Web Services