DICOM PS3.4 2018e - Service Class Specifications

CC.2.6.4 Status Codes (Current)
Prev | CC.2.6 Set Unified Procedure Step Information (N-SET) | Next

#### CC.2.6.4 Status Codes

Table CC.2.6-1 defines the status code values that might be returned in a N-SET response. General status code values and fields related to status code values are defined for N-SET DIMSE Service in PS3.7.

Table CC.2.6-1. Status Values

Service Status | Further Meaning | Status Code
--- | --- | ---
Success | The requested modification of the Attribute values is performed | 0000
Warning | Requested optional Attributes are not supported. | 0001
Coerced invalid values to valid values | B305
Failure | Failed: The UPS is not in the "IN PROGRESS" state | C310
Failed: The correct Transaction UID was not provided | C301
Failed: The UPS may no longer be updated | C300
Failed: Specified SOP Instance UID does not exist or is not a UPS Instance managed by this SCP | C307

Prev | Up | Next
CC.2.6.3 Service Class Provider Behavior | Home | CC.2.7 Get Unified Procedure Step Information (N-GET)

DICOM PS3.4 2018e - Service Class Specifications