DICOM PS3.3 2018e - Information Object Definitions

A.8.3.4 Multi-frame Grayscale Byte SC Image IOD Content Constraints (Current)
Prev | A.8.3 Multi-frame Grayscale Byte Secondary Capture Image IOD | Next

#### A.8.3.4 Multi-frame Grayscale Byte SC Image IOD Content Constraints

The VOI LUT Module is required if the VOI LUT stage is not an identity transformation. Support for both window and LUT is mandatory. The output grayscale space is defined to be in P-Values.

### Note

If the VOI LUT Module is absent, then the stored pixel values are in P-Values.

In the Image Pixel Module, the following constraints apply:

- Samples per Pixel (0028,0002) shall be 1

- Photometric Interpretation (0028,0004) shall be MONOCHROME2

- Bits Allocated (0028,0100) shall be 8

- Bits Stored (0028,0101) shall be 8

- High Bit (0028,0102) shall be 7

- Pixel Representation (0028,0103) shall be 0

- Planar Configuration (0028,0006) shall not be present

- Rescale Intercept shall be 0

- Rescale Slope shall be 1

- Rescale Type shall be US

The Overlay Plane Module shall not be present.

Prev | Up | Next
A.8.3.3 Multi-frame Grayscale Byte SC Image IOD Module Table | Home | A.8.3.5 Multi-frame Grayscale Byte SC Image Functional Group Macros

DICOM PS3.3 2018e - Information Object Definitions