DICOM PS3.16 2018e - Content Mapping Resource

TID 4013 Mammography CAD Selected Region (Current)
Prev | Mammography CAD SR IOD Templates | Next

### TID 4013 Mammography CAD Selected Region

This Template provides the detail specific to a selected region. A selected region is any mammography CAD derived arbitrary region of the image, whether within the breast outline or not. This can be use to delineate regions such as the intramammary fold.

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4013. Mammography CAD Selected Region

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | TEXT | EV (111058, DCM, "Selected Region Description") | 1 | M |  |
2 |  |  | INCLUDE | DTID 1400 “Linear Measurement” | 1-n | U |  | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID 1400 “Linear Measurement” shall be used.
3 |  |  | INCLUDE | DTID 1401 “Area Measurement” | 1-n | U |  | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID 1401 “Area Measurement” shall be used.
4 |  |  | INCLUDE | DTID 1402 “Volume Measurement” | 1-n | U |  | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID 1402 “Volume Measurement” shall be used.

Prev | Up | Next
TID 4012 Mammography CAD Non-lesion | Home | TID 4014 CAD Image Quality

DICOM PS3.16 2018e - Content Mapping Resource