DICOM PS3.3 2018e - Information Object Definitions

C.7.6.18.3 Bulk Motion Synchronization Module (Current)
Prev | C.7.6.18 Physiological Synchronization | Next

##### C.7.6.18.3 Bulk Motion Synchronization Module

Table C.7.6.18-3 specifies the Attributes of the Bulk Motion Synchronization Module.

Table C.7.6.18-3. Bulk Motion Synchronization Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Bulk Motion Compensation Technique | (0018,9172) | 1C | Applied technique to reduce bulk or other physiology motion artifacts. Defined Terms: NONE REALTIME image acquisition shorter than motion cycle GATING prospective gating TRACKING prospective through and/or in-plane motion tracking RETROSPECTIVE retrospective gating CORRECTION retrospective image correction Required if Image Type (0008,0008) Value 1 is ORIGINAL or MIXED. May be present otherwise.
Bulk Motion Signal Source | (0018,9173) | 1C | Signal source to measure motion. Defined Terms: JOINT joint motion detection NAVIGATOR MR navigator and organ edge detection MR_PHASE phase (of center k-space line) Required if Image Type (0008,0008) Value 1 is ORIGINAL or MIXED and Bulk Motion Compensation Technique (0018,9172) equals other than NONE. Otherwise may be present if Image Type (0008,0008) Value 1 is DERIVED and Bulk Motion Compensation Technique (0018,9172) equals other than NONE.

Prev | Up | Next
C.7.6.18.2 Respiratory Synchronization Module | Home | C.7.6.19 Supplemental Palette Color Lookup Table Module

DICOM PS3.3 2018e - Information Object Definitions