DICOM PS3.7 2019a - Message Exchange

C.5.10 Invalid Argument Value (Current)
Prev | C.5 Failure Status Class | Next

### C.5.10 Invalid Argument Value

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0115H.
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which an argument value was in error.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the ID of the SOP Instance for which an argument value was in error.
Event Type ID | (0000,1002) | US | 1 | This optional field contains the UID of the Event Type that was not recognized. Permitted only in the N-EVENT-RSP.
Event Information | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid argument values conveyed in the Event Information of the request. Permitted only in the N-EVENT-REPORT-RSP.
Action Type ID | (0000,1008) | US | 1 | This optional field contains the ID of the Action Type that was not recognized. Permitted only in the N-ACTION-RSP.
Action Information | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid argument values conveyed in the N-ACTION-RQ. Permitted only in the N-ACTION-RSP.

Prev | Up | Next
C.5.9 Duplicate Invocation | Home | C.5.11 Invalid Attribute Value

DICOM PS3.7 2019a - Message Exchange