DICOM PS3.3 2019a - Information Object Definitions

A.52.4.3 Ophthalmic Tomography Image Functional Group Macros (Current)
Prev | A.52.4 Ophthalmic Tomography Image IOD Content Constraints | Next

#### A.52.4.3 Ophthalmic Tomography Image Functional Group Macros

Table A.52.4.3-1 specifies the use of the Functional Group Macros used in the Multi-frame Functional Groups Module for the Ophthalmic Tomography Image IOD.

Table A.52.4.3-1. Ophthalmic Tomography Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Pixel Measures | C.7.6.16.2.1 | M
Frame Content | C.7.6.16.2.2 | M - May not be used as a Shared Functional Group.
Plane Position (Patient) | C.7.6.16.2.3 | C - Required if no Ophthalmic Photography Reference Image is available or if Ophthalmic Volumetric Properties Flag (0022,1622) is YES; May be present otherwise
Plane Orientation (Patient) | C.7.6.16.2.4 | C - Required if no Ophthalmic Photography Reference Image is available or if Ophthalmic Volumetric Properties Flag (0022,1622) is YES; May be present otherwise
Referenced Image | C.7.6.16.2.5 | C - Required if Ophthalmic Photography Reference Image is available.
Derivation Image | C.7.6.16.2.6 | C - Required if the image or frame has been derived from another SOP Instance.
Frame Anatomy | C.7.6.16.2.8 | M
Cardiac Synchronization | C.7.6.16.2.7 | C - Required if Cardiac Synchronization Technique (0018,9037) equals other than NONE. May be present otherwise.
Contrast/Bolus Usage | C.7.6.16.2.12 | C - Required if Contrast/Bolus Agent Sequence (0018,0012) is used. May not be used as a Shared Functional Group
Ophthalmic Frame Location | C.8.17.10.1 | U

Prev | Up | Next
A.52.4.2 Overlay Plane Module and VOI LUT Module | Home | A.53 X-Ray 3D Angiographic Image IOD

DICOM PS3.3 2019a - Information Object Definitions