DICOM PS3.3 2019a - Information Object Definitions

C.11.16 Structured Display Module (Current)
Prev | C.11 Look Up Tables and Presentation States | Next

### C.11.16 Structured Display Module

Table C.11.16-1 describes the Attributes of the Structured Display Module.

Table C.11.16-1. Structured Display Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Include Table 10-12 “Content Identification Macro Attributes” |
Presentation Creation Date | (0070,0082) | 1 | Date on which this structured display was created. ### Note This date may be different from the date that the DICOM SOP Instance was created, since the structured display information contained may have been recorded earlier.
Presentation Creation Time | (0070,0083) | 1 | Time at which this structured display was created. ### Note This time may be different from the time that the DICOM SOP Instance was created, since the structured display information contained may have been recorded earlier.
Number of Screens | (0072,0100) | 1 | The number of screens for this Structured Display. If SOP Class UID (0008,0016) equals 1.2.840.10008.5.1.4.1.1.131(Basic Structured Display), the value shall be 1.
Nominal Screen Definition Sequence | (0072,0102) | 1 | Sequence of Items that describes the set of screens for this Structured Display. The number of Items shall equal the value of Number of Screens (0072,0100). One or more Items shall be included in this Sequence. ### Note The Basic Structured Display IOD limits this Sequence to one Item.
>Include Table C.23.2-2 “Screen Specifications Macro Attributes” |
Icon Image Sequence | (0088,0200) | 3 | This icon image is representative of the structured display. Only a single Item is permitted in this Sequence.
>Include Table C.7-11b “Image Pixel Macro Attributes” | See Section C.7.6.1.1.6 for further explanation.
Structured Display Background CIELab Value | (0072,0420) | 3 | A value in which it is recommended that Structured Display background (i.e., the area outside of Image Boxes) be rendered on a color display. The units are specified in PCS-Values, and the value is encoded as CIELab. See Section C.10.7.1.1.
Empty Image Box CIELab Value | (0072,0421) | 3 | A value in which it is recommended that empty Image Boxes be rendered on a color display. The units are specified in PCS-Values, and the value is encoded as CIELab. See Section C.10.7.1.1.
Hanging Protocol Name | (0072,0002) | 3 | Identifies the hanging protocol that was used in the creation of this structured display. See Table OO.1.1-1 “Hanging Protocol Names for Dental Image Layout based on JSOMR classification” in PS3.17 for standard hanging protocols for dentistry.
Hanging Protocol Creator | (0072,0008) | 3 | Identifies the creator of the Hanging Protocol. See Table OO.1.1-1 “Hanging Protocol Names for Dental Image Layout based on JSOMR classification” in PS3.17 for standard hanging protocols for dentistry.

Prev | Up | Next
C.11.15 ICC Profile Module | Home | C.11.17 Structured Display Image Box Module

DICOM PS3.3 2019a - Information Object Definitions