DICOM PS3.4 2019a - Service Class Specifications

5.3 Response Status Values (Current)
Prev | 5 Conventions | Next

## 5.3 Response Status Values

Certain tables in this Part of the DICOM Standard denote an implementation specific response status code by using the symbol 'xx' or 'xxx' as part of the code.

### Note

Each 'x' symbol may be replaced by an implementation with a hexadecimal digit in the range from 0 to F.

Prev | Up | Next
5.2 Sequences | Home | 5.4 Usage Specification

DICOM PS3.4 2019a - Service Class Specifications