DICOM PS3.2 2019a - Conformance

G.8.4 Grayscale Image Consistency (Current)
Prev | G.8 Annexes | Next

### G.8.4 Grayscale Image Consistency

The high resolution display monitor attached to the product can be calibrated according to the Grayscale Standard Display Function (GSDF).

Prev | Up | Next
G.8.3 Coded Terminology and Templates | Home | G.8.5 Standard Extended/Specialized/Private SOP Classes

DICOM PS3.2 2019a - Conformance