DICOM PS3.18 2019a - Web Services

6.9.5 ChangeUPSState (Current)
Prev | 6.9 UPS-RS Worklist Service | Next

### 6.9.5 ChangeUPSState

This resource supports the modification of the state of an existing UPS Instance.

#### 6.9.5.1 Request

The request message shall be formed as follows:

- Resource

  - {+SERVICE}/workitems/{UPSInstanceUID}/state

    where:

    - {+SERVICE} is the base URL for the service. This may be a combination of protocol (either HTTP or HTTPS), authority and path.

    - {UPSInstanceUID} is the UID of the Unified Procedure Step Instance

- Method

  - PUT

- Headers

  - Content-Type - The representation scheme being posted to the RESTful service. The types allowed for this request header are as follows:

    - application/dicom+xml

      Specifies that the post is DICOM PS3.19 XML metadata. See Section 6.9.5.1.1.

    - application/dicom+json

      Specifies that the post is DICOM PS3.18 JSON metadata. See Section 6.9.5.1.1.

- The request body describes a state change to a single Unified Procedure Step Instance. It shall include all Attributes required for an SCU in Table CC.2.1-1 in PS3.4 .

##### 6.9.5.1.1 Request Message

The Request Message has a single part body.

- Content-Type:

  - application/dicom+xml

  - application/dicom+json

- The request body contains attributes in either DICOM PS3.19 XML or DICOM PS3.18 JSON format.

Prev | Up | Next
6.9.4.3.2 Response Message | Home | 6.9.5.2 Behavior

DICOM PS3.18 2019a - Web Services